;;	EditText.dat
;;
;;	2007/7/20

[SELECT_PARTS_DIALOG]
COUNT=1
TEXT1=Select from the chart below the parts you replaced or remove and click the OK button. The required adjustments will automatically be decided and the correct order in which they are to be performed will be displayed.

[STATUS_MONITOR]
BitmapFile1=prnidle.bmp
BitmapFile2=prnerror.bmp

[INDIVIDUAL_LIST]
COUNT=1
TEXT1=Select an adjustment item from the below window and double-click to execute it.

[EEPROM_COPY]
COUNT=4
TEXT1=This function copies EEPROM data from current main board to new main board.
TEXT2=1) Click [Backup] button to backup EEPROM data from current main board.
TEXT3=2) Turn off the printer and replace current main board with new one.
TEXT4=3) Reboot the printer and click [Restore] button.

[EEPROM_INITIALIZE]
COUNT=6
TEXT1=NOTE : Please don't execute this function when backing up the EEPROM data
TEXT2=       with EEPROM Data Copy function.
TEXT3=
TEXT4=1) Click [Initial setting] button to write initial setting value to EEPROM.
TEXT5=2) Input the Product Serial No. and click the [USB-ID input] button to write the new USB-ID to EEPROM.
TEXT6=3) Click the [Check] button to read out current setting values.

[PF_DETERIORATION_OFFSET]
COUNT=1
TEXT1=1) Click [Initialization] button to reset current PF offset value to "Zero".

[PF_DETERIORATION_OFFSET_MAX]
COUNT=1
TEXT1=1) Click [Input] button to set the maximum PF offer value into EEPROM.

[HEAD_ID_INPUT]
BitmapFile1=headid.bmp
COUNT=7
TEXT1=[Method to input the Head ID]
TEXT2=1) Input Head ID in the edit box.
TEXT3=2) Click [Input] button to recorded Head ID into EEPROM.
TEXT4=     If error message is displayed, please input Head ID again.
TEXT5=
TEXT6=[How to check current Head ID]
TEXT7=1) Click [Check] button to check current Head ID.

[TOF_ADJUSTMENT]
COUNT=9
TEXT1=1) Place 4x6 size of Photo Paper Glossy(EAI)/Glossy Photo Paper(Euro/Asia) in the ASF.
TEXT2=2) Click [Print] button to print check pattern.
TEXT3=3) Measure the distance between the edge of paper and printed line.
TEXT4=4) Select the proper adjustment value from the measurement result.
TEXT5=5) Click [Input] button to record the selected value into EEPROM.
TEXT6=
TEXT7=[How to select the best line]
TEXT8=1) The printed line on should be 5mm away from each of the paper's edges.
TEXT9=2) Choose the selected pattern from edit box.

[BM_ADJUSTMENT]
COUNT=9
TEXT1=1) Place A4 size Matte Paper-Heavyweight in the ASF.
TEXT2=2) Click [Print] button to print check pattern.
TEXT3=3) Measure the distance between the edge of paper and printed line.
TEXT4=4) Select the proper adjustment value from the measurement result.
TEXT5=5) Click [Input] button to record the selected value into EEPROM.
TEXT6=
TEXT7=[How to select the best line]
TEXT8=1) The printed line on should be 5mm away from each of the paper's edges.
TEXT9=2) Choose the selected pattern from edit box.

[HEAD_ANGULAR]
COUNT=7
TEXT1=1) Place A4 size Plain Paper in the ASF.
TEXT2=2) Click [Print] button to print check pattern.
TEXT3=       - Band Pattern
TEXT4=       - Raster Offset Pattern
TEXT5=3) Select the number of the pattern with the best alignment from the list.
TEXT6=4) Choose the selected pattern from the edit box.
TEXT7=5) Click [Input] button to record the parameter into EEPROM.

[MANUAL_BID]
COUNT=9
TEXT1=1) Place A4 size Plain Paper in the ASF.
TEXT2=2) Click [Print] button to print check pattern of selected PG & selected dot size.
TEXT3=3) Select the number of the pattern with the best alignment from the list.
TEXT4=4) Choose the selected pattern from the edit box.
TEXT5=5) Click [Input] button to record the parameter to the EEPROM.
TEXT6=    For the case where there is no best pattern, you should input the maximum or
TEXT7=     minimum parameter of the test pattern which ever is most appropriate.
TEXT8=     The offset value will be printed in the center position the next time the check pattern is printed.
TEXT9=     Please repeat this adjustment until you can select the best pattern.

[PW_ADJUSTMENT]
COUNT=9
TEXT1=1) Place A4 size Economy Photo Paper/Glossy Photo Paper in the ASF.
TEXT2=2) Click [Print] button to print check pattern.
TEXT3=3) Select the number of the pattern with the best alignment from the list.
TEXT4=4) Choose the selected pattern from the edit box.
TEXT5=5) Click [Input] button to record the parameter to the EEPROM.
TEXT6=
TEXT7=[How to select the best line]
TEXT8=1) The printed line on should be 5mm away from each of the paper's edges.
TEXT9=2) Choose the selected pattern from edit box.

[FIRST_DOT]
COUNT=9
TEXT1=1) Place A4 size Matte Paper-Heavyweight in the ASF.
TEXT2=2) Click [Print] button to print check pattern.
TEXT3=3) Select the number of the pattern with the best alignment from the list.
TEXT4=4) Choose the selected pattern from the edit box.
TEXT5=5) Click [Input] button to record the parameter to the EEPROM.
TEXT6=
TEXT7=[How to select the best line]
TEXT8=1) The printed line on should be 5mm away from each of the paper's edges.
TEXT9=2) Choose the selected pattern from edit box.

[PF_ADJUSTMENT]
COUNT=5
TEXT1=1) Place A4 size Matte Paper-Heavyweight in the ASF.
TEXT2=2) Click [Print] button to print check pattern.
TEXT3=3) Select the number of the pattern with the best alignment from the list.
TEXT4=4) Choose the selected pattern from the edit box.
TEXT5=5) Click [Input] button to record the parameter to the EEPROM.

[PF_BAND_ADJUSTMENT]
COUNT=5
TEXT1=1) Place A4 size Plain Paper in the ASF.
TEXT2=2) Click [Print] button to print check pattern.
TEXT3=3) Select the number of the pattern with the best alignment from the list.
TEXT4=4) Choose the selected pattern from the edit box.
TEXT5=5) Click [Input] button to record the parameter to the EEPROM.

[HEAT_PROTECTION]
BitmapFile1=Caution.bmp
COUNT=6
TEXT1=1) Select replacement parts from the following check boxes.
TEXT2=    Please do not perform this adjustment prior to replacing the affected parts
TEXT3=    with new one.
TEXT4=2) Click [Perform] button to record the proper value of CR motor heat protection
TEXT5=    to EEPROM for the selected replacement parts. (This operation,
TEXT6=    it takes about 1 min.)

[BRS_ADJUSTMENT]
COUNT=7
TEXT1=1) Print Test Pattern
TEXT2=   Set an A4 size Matte Paper-Heavyweight in the ASF, then click the [Print] button.
TEXT3=Note : Please let the printed pattern dry for more than five minutes before scanning it with an CIS sensor type scanner.
TEXT4=
TEXT5=2) Scan Test Pattern
TEXT6=   Select the scanner you want to use from the list box.
TEXT7=   Then set the PFP Base Scale & Test Pattern on the document table, and click the [Perform] button.

[PFP_ADJUSTMENT]
COUNT=10
TEXT1=1) Print Test Pattern
TEXT2=   Set a 4 x 6 size Premium Glossy Photo Paper on the ASF, then click the [Print] button.
TEXT3=
TEXT4=2) Scan Test Pattern
TEXT5=   Select the scanner you want to use from the list box.
TEXT6=   Set the PFP Base Scale & Test Pattern on the document table, then click the [Scan] button.
TEXT7=
TEXT8=3) Print Check Pattern
TEXT9=   Set a 4 x 6 size Premium Glossy Photo Paper on the ASF, then click the [Print] button.
TEXT10=   Then check and judge the printed-pattern by referring to the service manual.

[CLEANING]
COUNT=4
TEXT1=1) Click [Print] button to print nozzle check pattern print.
TEXT2=2) If dot missing appears, click [Cleaning] button to perform a cleaning.
TEXT3=3) Click [Print] button to print nozzle check pattern print again.
TEXT4=4) If dot missing is not recovered, repeat from step 2) to step 3)

[INK_CHARGE]
COUNT=5
TEXT1=1) Click [Ink Charge] button to perform ink charge.
TEXT2=2) Click [Print] button to print nozzle check pattern print.
TEXT3=3) If dot missing appears, click [Cleaning] button to perform a cleaning.
TEXT4=4) Click [Print] button to reprint nozzle check pattern
TEXT5=5) If dot missing is not recovered, repeat from step 3) to step 4)

[INK_PAD_COUNTER]
COUNT=6
TEXT1=NOTE : You have to replace waste ink pad if you initialize
TEXT2=             the protection counter.
TEXT3=
TEXT4=1) Click [Check] button to check current protection counter's value.
TEXT5=2) Replace waste ink pad with new one.
TEXT6=3) Click [Initialization] to reset the protection counter to the initial value.

[SHIPPING_SETTING]
COUNT=5
TEXT1=This function will have a cleaning process performed automatically when the printer is turned on.
TEXT2=1) Please use this function in case of nozzle clogging  during transport. After clicking the "Write" button, the shipping settings will be written to the devise.
TEXT3=2) The shipping settings will be recorded when the printer is turned off and applied automatically the next time it is turned on.
TEXT4=Attention:
TEXT5=This function resets the shipping settings if the printer is turned on. In this situation, it is necessary to reset the shipping settings once again before turning off the power.

[CHECK_PATTERN_PRINT]
COUNT=1
TEXT1=1) Click [Print] button to print selected pattern.

[CDR_CHKPAT_PRINT]
COUNT=1
TEXT1=1) Click [Print] button to print CD-R check pattern.

[EEPROM_READOUT]
COUNT=1
TEXT1=1) Click [Dump] button to read out and save all of EEPROM data.

[OPERATION_INFO]
COUNT=1
TEXT1=1) Click the [Check] button to read out the printer information.

[INK_DISCHARGE]
COUNT=4
TEXT1=1) Use the Jig.
TEXT2=2) Use the shipping liquid (CR02)
TEXT3=3) Click the [Perform] button to start the discharge.
TEXT4=4) Please discharge the shipping liquid outside of the printer when you execute this function. Otherwise ink may leak from the waste ink pad at user side.
